
SDM-6000 Update


2/12/16

1. Turn ON the SDM-6000 and connect it to the PC using a USB cable.
2. Start up “SDM6000Upd2.exe”.
3. Select the SDM-6000’s COM port.
4. Click the “…” button and navigate to the location of the latest .bin file.
5. Click Start and then click OK in the window that pops up.


If you get an error message before the OK window pops up, restart the SDM6000Upd2 program, reconnect the SDM-6000, make sure there are no IrDA devices plugged in, and make sure there are no other programs running.



1. Once the update is completed, the following message appears. Click OK and then turn the SDM-6000 off and then on again.



1. IF the LED is green and there is no red “x” at the bottom of the Function Tab once the SDM-6000 has restarted, the programming is complete and you may disconnect the SDM-6000 from the computer.
2. IF the LED is red and there is a red “x” at the bottom of the Function Tab once the SDM-6000 has restarted, open SDM6000SS.exe.



1. Select the SDM-6000’s COM port and click the Default button.